GETTING YOUR VEHICLE READY FOR SUMMER

     Summer's heat, dust, and stop-and-go traffic will take
their toll on your vehicle. Add the effects of last winter, 
and you could be poised for a breakdown. You can lessen the 
odds of mechanical failure through periodic 
maintenance...Your vehicle should last longer and command a 
higher resale price, too!

     Some of the following tips are easy to do; others 
require a skilled auto technician.

Getting Started--The best planning guide is your owner's
manual. Read it; and follow the manufacturer's recommended
service schedules.

   * Air Conditioning--A Marginally operating system will 
     fail in hot weather. Have the system examined by a 
     qualified technician.

   * Cooling System--The greatest cause of summer 
     breakdowns is overheating. The cooling system should 
     be completely flushed and refilled about every 24 
     months. The level, condition, and concentration of the 
     coolant should be checked periodically. (A 50/50 mix 
     of anti-freeze and water is usually recommended.)

          DIYers, Never remove the radiator cap until the 
engine has thoroughly cooled! The tightness and condition 
of drive belts, clamps, and hoses should be checked by a 
pro.

   * OIL--Change your oil and oil filter as specified in 
     your manual--more often (every 3,000 miles) if you 
     make frequent short jaunts, extended trips with lots 
     of luggage, or tow a trailer.

   * Engine Performance--Replace other filters (air, fuel, 
     PCV, etc.) as recommended--more often in dusty 
     conditions. Get engine driveability problems (hard 
     starts, rough idling, smiling, diminished power, etc.) 
     corrected at a good shop.

   * Windshield Wipers--A dirty windshield causes eye 
     fatigue and can pose a safety hazard. Replace worn 
     blades and get plenty of windshield washer solvent.

   * Tires--Have your tires rotated about every 5,000 
     miles.  Check tire pressures once a month; let the 
     tires "cool down" first.

          Don't forget your spare, and be sure the jack is 
in good condition. Examine tires for tread life, uneven
wearing, and cupping; check the sidewalls for cuts and
nicks. An alignment is warranted if there's uneven tread
wear or if your vehicle pulls to one side.

   * Brakes--Brakes should be inspected as recommended in 
     your manual, or sooner if you notice pulsations, 
     grabbing, noises, or longer stopping distance. Minor 
     brake problems should be corrected promptly.

   * Battery--Batteries can fail any time of year. The only
     accurate way to detect a weak battery is with 
     professional equipment. Routine care: Scrape away 
     corrosion from posts and cable connections; clean all 
     surfaces; re-tighten all connections. If battery. caps 
     are removable, check the fluid level monthly.

          Avoid contact with corrosive deposits and battery
     acid. Wear eye protection and rubber gloves.

   * Lights--Inspect all lights and bulbs; replace burned 
     out bulbs; periodically clean dirt and insects from 
     all lenses.

     To prevent scratching, never use a dry rag.

   * Emergencies--Carry some basic tools--ask a technician 
     for suggestions. Also include a first aid kit, flares, 
     and a flashlight. Consider buying a CB radio.